**DESCRIPTION**

* Powerful air flow and quiet operation - Cools rooms up to 350 sq. ft. (Temperature range 61oF to 89oF)
* Auto Evaporation – no bucket to empty (except in areas with high humidity), long-lasting Washable Dust Filter, Quick & Easy installation (Exhaust hose length: 12” to 47”, Window Bracket Width: Min. 19.7” to 47.2”)
* Washable filter & Filter Change Alert for easy maintenance
* Built-in Dehumidifier removes up to 44 pints/ 24 hours with continuous drain option for longer unattended operation
* 2 speeds, digital controls, 24 hour energy saving timer & remote control included